

[bookmark: _yatqy74c9nvc]NVR H2D16PAC (16-ch)

[bookmark: _cz6mkvy5gci]16-channel network video recorder with 4K HDMI output, 16 PoE ports, and support for 2 hot-swappable HDDs
	[bookmark: _twov7kfp0uel]Video
	Video input
16 channels

Recording resolution
12 MP, 8 MP, 6 MP, 5 MP, 4 MP, 3 MP, 1080p, UXGA, 720p, VGA, 4CIF, DCIF, 2CIF, CIF, QCIF

HDMI output resolution
3840 × 2160, 1920 × 1080, 1280 × 1024, 1280 × 720 px

Live view / playback resolution
12 MP, 8 MP, 6 MP, 5 MP, 4 MP, 3 MP, 1080p, 720p, D1, VGA, CIF

	[bookmark: _jfndqvwvzllu]Decoding
	Format
H.265, H.264, JetSparrow

Live view window division
templates: 1, 4, 9, 16, 25, 5+1, 7+1, 12+1 views
custom: up to 10×10 views

Synchronous playback
4 channels

	[bookmark: _1l7evu9wipha]Intelligent video analytics
	Motion detection
Ajax camera: 16 channels
NVR: 16 channels
NVR features built-in software to detect movement in the frame. It is possible to switch between image analysis by NVR or camera algorithms in an Ajax app.

AI-powered object detection
Ajax camera: 16 channels

	[bookmark: _ekzrhro0ohf]Interface
	HDD
2 × SATA III: supports hard drives with up to 16 TB capacity (2.5" and 3.5" form factors)
Supports full hot-swap functionality. HDDs are not included.

Network
1 × RJ45 self-adaptive Ethernet (10/100/1000 Mbps)
16 × 802.3af/at PoE RJ45 fast Ethernet (10/100 Mbps)

USB
rear panel: 2 × USB 2.0 (Type-A)
For connecting a keyboard, mouse, or USB Audio Device Class devices (Audio IN/Audio OUT).
front panel: 1 × USB 2.0 (Type-A)
To connect a USB flash drive.

	[bookmark: _ekzrhro0ohf]PoE standard
	PoE port
16 × IEEE 802.3af/at (Alternative A, power over data pairs)

Maximum power per port
up to 25 W

Total power budget
up to 160 W

	[bookmark: _9g64ez41mmra]Network
	Bandwidth
incoming: up to 160 Mbps
outgoing: up to 160 Mbps

Protocol
HTTP, HTTPS, TCP/IP, IPv4, IPv6, UPnP, SNMP, RTSP, UDP, SMTP, NTP, DHCP, DNS, DDNS

Interoperability
ONVIF

	[bookmark: _jfndqvwvzllu]Key features
	Supported devices
· Ajax cameras
· IP cameras via ONVIF (Profile S/T) or RTSP

Redundancy mode
Simultaneous recording of the same video streams to two storage devices to ensure data redundancy and reliability.

Split mode
Sequentially distributes video streams across multiple storage devices to balance the load and optimize storage.

Built-in video management system
· Integrated video wall interface with live camera feeds.
· Smart event filters for quick access to relevant video recordings.
· Interactive timeline with preview navigation for efficient playback and incident review.

Visual verification of Ajax system alarms
NVR supports a scenario in which events triggered by Ajax detectors automatically highlight the corresponding camera feed on the video wall. This allows an operator to immediately verify the intrusion.

Privacy
Advanced privacy controls ensure a high level of personal data protection. All access rights — including those for mobile app users, installers, and monitoring company operators via Ajax PRO Desktop — are fully configurable by the device owner. This guarantees that only authorized parties can access video streams, event history, or device settings in accordance with the owner's preferences.

Accelerometer
alarm when NVR is moved

	[bookmark: _9vfm0f92m9sw]Recommendations
	The device's operating voltage is 100–240 V~.
The device is designed for indoor installation only.

	[bookmark: _jfndqvwvzllu]Power supply
	Main
100–240 V, 50/60 Hz, 5 A

Power consumption
up to 280 W

Clock battery
CR2032 battery, 3 V
Only to power the system clock.

	[bookmark: _jfndqvwvzllu]Enclosure
	Dimensions
330 × 330 × 44 mm
12.99″ × 12.99″ × 1.73″

Weight
3.3 kg
7.3 lb
Without hard drives.

Operating temperature range
from 0 °C to +50 °C
from 32 °F to 122 °F

Operating humidity
up to 75%

Protection class
IP20
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	Black
White


	[bookmark: _jfndqvwvzllu]Complete set
	NVR H2D16PAC (16-ch)
2 × rack-mount brackets
Power cable
Ethernet cable
Installation kit
Quick start guide

	Warranty
	24 months





